**COB ULTRA LED SERIES**

**SUPERB VISUAL IMPACT**

Contrast with 6000:1

Deep Black and Vibrant colors

Easy to handle and maintain

Perfectly coated led to Interact Applications

**SEAMLESS SPLICING**

Each COB series are seamlessly connected for a longer indoor application and display a sharp view.

Its an Ultra HD display with COB to protect from dust and moisture.

With <0.2mm tolerance

**PLUGNPLAY HANDLING**

Ultra-viewing angle 160

Frontend installation and maintenance

Wall mounting and Stacking

**INDUSTRIAL OUTLET APPLICATIONS**

Ultra HD series suitable for Retail, Government, Corporate, Boardroom, Studios, Education platforms. Save time and labor back maintenance.

**Display Properties**

**Pixel Pitch** P1.25, P1.53, P1.86, P2, P2.5

**Resolution** 640,000, 422,500, 288906,250,000, 160,000

**Brightness** , 700nits, 700nits, 700nits, 700nits, 1000nits

**Refresh Rate** 3840Hz, 3840Hz, 3840Hz, 3840Hz

**Contrast** 6000:1, 6000:1, 6000:1, 6000:1

**Color Depth** 16bit

**Viewing Angle (h/v)** 120/120

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Indoor - DieCasting

**Operating Temperature** -20/60, -20/60, -20/60, -20/60

**Operating Humidity**  0 to 70%

**Environment Rating** IP45, IP40, IP45, IP45,

**Weight** 16.5Ib

**Weight Metric** 7.5Kg

**Dimensions** 2.1ft\*1.57ft

**Dimensions Metric** 640\*480mm

**Panel Power (Max/Avg)** 580/w

**Build**

**Installation & Service** Front

**Operating Voltage** AC 100 – 240V

**Certifications** CE, RoHS, CCC, FCC