**INDOOR FIXED SERIES**

**CUSTOMIZED CABINET DESIGN**

Featuring the Black LEDs,

Modular cabinet design

Customizable sizes available according to modules

**HIGH STRENGTH**

General cabinet sizes 960\*960, 960\*480, 1280\*960, 640\*960

Easy to Handle and rare maintenance

High Strength structure, embedded receiver

Advanced color calibration

**BETTER FLATNESS**

Intelligently hooks to handle

Safer design, fixed on the wall

Multi-functional handling

**SPECIAL CABINET HEAT DESSIPATION**

This design a specific location of power supply makes it colder

Prevents to store heat inside

**Display Properties**

**Pixel Pitch** P3, 4, 5,6, 10

**Resolution** 64\*64, 64\*32, 64\*32, 32\*32, 32\*16

**Brightness** 900nits, 1000nits, 1600nits, 2200nits, 1800nits

**Refresh Rate** 1920Hz,

**Contrast** n/a, n/a, n/a, n/a, n/a, n/a

**Color Depth** 14bit

**Viewing Angle (h/v)** 140/140

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Indoor, Outdoor

**Operating Temperature** -10 ~ 1000 F

**Operating Humidity**  0 to 80%

**Environment Rating** Ip45, ip45, ip45, ip65, ip65

**Weight** OEM

**Weight Metric** OEM

**Dimensions** OEM

**Dimensions Metric** OEM

**Panel Power (Max/Avg)** 550

**Build**

**Installation & Service** Back Maintenance

**Operating Voltage** AC 100 – 240V

**Certifications** CE, CCC, FCC