**iPoster led display**

**SLIM & LIGHT**

Slim, Ultra-thin frame

Each structure set weight 32KG

Easy to handle and maintain

**FRONT SERVICE**

LED Screen panels

Can build standard resolution HD, FHD, 2k, 4k,

Easy to Handle and maintenance

Seamlessly connectivity

**PROTECTION & INTERFACE**

Ultra-bright, adjustable with dual mode.

Multifunctioning Interface

Standing, Wall mounted, Hoisting installation

**PLUGNPLAY CONTROL**

iPoster easy to use just plug n play

Can relate to Wi-Fi, 4G, 5G, Screen mirroring

Seamless splicing

**Display Properties**

**Pixel Pitch** P2.5, 3

**Resolution** 196608, 122880

**Brightness** 800nits, 800nits

**Refresh Rate** 1920

**Contrast** 5000:1, 5000:1, 5000:1

**Color Depth** 16bit

**Viewing Angle (h/v)** 140/140

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Indoor

**Operating Temperature** -10 ~ 1000 F

**Operating Humidity**  0 to 80%

**Environment Rating** Ip45

**Weight** 70 Ib

**Weight Metric** 32Kg, 32Kg\

**Dimensions** 6.3ftx2.1ft

**Dimensions Metric** 1920x640mm

**Panel Power (Max/Avg)** 150W

**Build**

**Installation & Service** Front

**Operating Voltage** AC 100 – 240V

**Certifications** CE, CCC, FCC