**OUTDOOR FIXED SERIES**

**HIGH COMPATIBILITY**

General cabinet sizes 960\*960, 960\*480, 1280\*960, 640\*960

Easy to Handle and rare maintenance

High Strength structure, embedded receiver

Advanced color calibration

**EASY FIXED**

8 holes connectivity support for rear and front

Build in wire

Dual Maintenance

Partition design for control box

Control box and wire box and independent

**BETTER FLATNESS**

Intelligently hooks to handle

Safer design, fixed on the wall

Multi-functional handling

**SPECIAL CABINET HEAT DESSIPATION**

This design a specific location of power supply makes it colder

Prevents to store heat inside

**Display Properties**

**Pixel Pitch** P4, 5,6.6, 8,10

**Resolution** 240\*240, 192\*192, 144\*144, 120\*120, 96\*96

**Brightness** 6000nits, 6500nits, 7000nits, 7000nits, 7000nits

**Refresh Rate** 1920Hz, 3840Hz

**Contrast** n/a, n/a, n/a, n/a, n/a, n/a

**Color Depth** 14bit

**Viewing Angle (h/v)** 160/120

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Outdoor

**Operating Temperature** -10 ~ 1000 F

**Operating Humidity**  0 to 80%

**Environment Rating** Ip65

**Weight** 70.5Ib

**Weight Metric** 32Kg

**Dimensions** 3.15ft\*3.15ft

**Dimensions Metric** 960\*960mm

**Panel Power (Max/Avg)** 750/250

**Build**

**Installation & Service** Front &Back Maintenance

**Operating Voltage** AC 100 – 240V

**Certifications** CE, CCC, FCC