**3D Hologram Fan**

**CLOUD MANAGEMENT**

3d Hologram Display provides a free Cloud server for customers. Can control the devices anytime anywhere around the world.

**GROUP MANAGEMENT**

Iledscreen 3D Fan can group 2 or more pieces fans in one group, upload one video at a time.

Saving time.

**APP CONTROL**

Fan Display can control by Android and iPhone App, customers can easily control it anytime.

User-friendly platform.

Supports web platform management for advertising business, easy to manage on a big screen

**Display Properties**

**Pixel Pitch** 50A, 70A, 43A

**Resolution** 500000, 1200000, 100800

**Brightness** , 1600nits

**Refresh Rate** N/A

**Contrast** 5000:1

**Color Depth** 14bit

**Viewing Angle (h/v)** 140

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Indoor

**Operating Temperature** -10/35, -20/60, -20/60, -20/60

**Operating Humidity**  0 to 70%

**Environment Rating** IP45, IP40, IP45, IP45,

**Weight** 3.6Ib, 2.5LB, 2.4LB

**Weight Metric** 1.65Kg, 1.7KG, 1.6KG

**Dimensions** 1.6ft\*1.6ft\*0.3FT, 2.29\*2.29\*0.32FT, 1.41\*0.43\*0.36FT

**Dimensions Metric** 500\*500\*100MM, 700\*700\*110MM, 430\*130\*110MM

**Panel Power (Max/Avg)** 70/w, 140w, 15W

**Build**

**Installation & Service** Front/BACK

**Operating Voltage** AC 100 – 240V

**Certifications** CE, CCC