**Iledscreen special tile series**

**ULTRA SLIM & LIGHT**

Capable of feature Plug n Play

Thickness to 40mm

Easy to handle and maintain

Perfectly coated led to Interact Applications

**WIRELESS CONNECTIONS**

Simpler inner structure

Easy maintenance

Dual backup of power supply

**QUICK AND EASY**

Front maintenance

No reserve spaces

End to end fixed and seamless effect

Support tacking installation, Hanging, Wall-mounted, Ceiling

**Retail Outlet Applications**

Its placed-on Hanging, Wall-mounted in the stores to help promote inventory in video advertisement. Best for Hanging in Exhibitions, Meetings, Shopping Mall, Window advertising.

**Display Properties**

**Pixel Pitch** P1.95, 2.5, 2.6

**Resolution** 65746,32873, 49310

**Brightness** 800nits, 800nits, 800nits

**Refresh Rate** 3840Hz, 3840Hz, 3840Hz

**Contrast** 5000:1, 5000:1, 5000:1

**Color Depth** 16bit

**Viewing Angle (h/v)** 140/140

**Diode Type** SMD

**Engineering**

**Indoor/Outdoor**  Indoor Tile

**Operating Temperature** 6500k,

**Operating Humidity**  0 to 70%

**Environment Rating** IP43

**Weight** 8.8/6.61/7.7Ib, 8.8/6.61/7.7Ib, 8.8/6.61/7.7Ib

**Weight Metric** 4/3/3.5, 3, 4/3/3.5

**Dimensions** 28”x2.36”x1.18”

**Dimensions Metric** 1000/500/750

**Panel Power (Max/Avg)** 100/80/90

**Build**

**Installation & Service** Front

**Operating Voltage** AC 100 – 240V

**Certifications** CE, EMC, CCC, FCC