**COB Shelf Ribbons**

**COB Advantages**

Capable of feature Plug n Play

IP65 Waterproofing protection

Easy to handle and maintain

Perfectly coated led to Interact Applications

**Seamless Spicing**

Each COB series are seamlessly connected for a longer shelf application and displays a sharp view.

It's an Ultra HD display with COB to protect from dust and moisture.

**Quick and Easy Handling**

A simple, modular design with Hooks, screws, and magnets which allow fitting on any shelves or rack.

It supports wall-mounted and mobile stand installation, which can easily be installed.

**Retail Outlet Applications**

Its placed-on shelves or rack in the stores to help promote inventory in a video advertisement.

Save time and labor by updating prices digitally.

**Display Properties**

**Pixel Pitch** P1.2, P1.5, P1.8

**Resolution** 576\*48, 480\*40, 384\*32

**Brightness** 600nits, 600nits, 600nits

**Refresh Rate** 3840Hz, 3840Hz, 3840Hz

**Contrast** 5000:1, 5000:1, 5000:1

**Color Depth** 16bit

**Viewing Angle (h/v)** 140/110

**Diode Type** GOB

**Engineering**

**Indoor/Outdoor**  Indoor

**Operating Temperature** 40/14, 40/14,

**Operating Humidity**  0 to 60%

**Environment Rating** IP20

**Weight** 2.4Ib,

**Weight Metric** 1.1, 1.1, 1.1

**Dimensions** 28”x2.36”x1.18”

**Dimensions Metric** 720x60x30mm

**Panel Power (Max/Avg)** 40/14

**Build**

**Installation & Service** Rare

**Operating Voltage** AC 100 – 240V

**Certifications** CE, EMC, CCC, FCC